                	P R O F I L E  A R C H I V E                                   
		       ------------------------------                                         
                                                                                
                         CASH RESOURCES LTD.                                    
                                                                                
Label MUCHO  Magnetics ,Vetrical Gradient EM and Resistivity data.              
                                                                                
	Structure...                                                                   
                                                                                
	This archive contains the profile data for the  MUCHO AREA                     
	Project, The  file                                                             
	has a record length of 206 bytes.                                              
                                                                                
		The order of files on this CD are :                                           
                                                                                
		1) The PROFILE ARCHIVE, label by area (ascii)                                 
                                                                                
		2) Grids,for mag,cvg,resl9x,resm4p (geosoft grids)                            
      	                                                                         
        Values for each data type are recorded in adjacent fields.              
	The LENGTH of the data fields is noted.                                        
                                                                                
	Where data were missing or deleted, a marker or flag                           
	value of -9999 was inserted.                                                   
                                                                                
	To retain precision, some channels were multiplied by                          
	a constant prior to copying to tape. The MULTIPLIERS are                       
	recorded in the table below.                                                   
                                                                                
          Output scan rate             :    0.2 Seconds.                        
                                                                                
		         DATA RECORD STRUCTURE                                                
		         *********************                                                
                    LENGTH  SUB      MULT     DEFAULT                           
                                                                                
         Line      :   8                                                        
         Flight    :   3                                                        
         Date      :   6                                                        
         Time      :   8                                                        
         Manual    :   9    0.00      1000     -9999	Fiducials                  
         UTM_EARC  :   9    0.00      1.00     -9999	Easting                    
         UTM_NARC  :   9    0.00      1.00     -9999	Northing                   
         RALT_FLT  :   9    0.00     10.00     -9999	Radar Altimeter (m)        
         BALT_FLT  :   9    0.00     10.00     -9999	Barometric  Altimeter (m)  
         MAG_LEVL  :   9    0.00   1000.00     -9999	Total Field Magnetics Level
         PXG_CVG   :   9    0.00  10000.00     -9999	Caculated vertical gradient
         EM        :   9    0.00     10.00     -9999    865 Hz coplanar inphase 
         EM        :   9    0.00     10.00     -9999    865 Hz coplanar quadratu
         EM        :   9    0.00     10.00     -9999    935 Hz coaxial inphase (
         EM        :   9    0.00     10.00     -9999    935 Hz coaxial quadratur
         EM        :   9    0.00     10.00     -9999    4175 Hz coplanar inphase
         EM        :   9    0.00     10.00     -9999    4175 Hz coplanar quadrat
         EM        :   9    0.00     10.00     -9999    4600 Hz coaxial inphase 
         EM        :   9    0.00     10.00     -9999    4600 Hz coaxial quadratu
         EM        :   9    0.00     10.00     -9999    33000 Hz coplanar inphas
         EM        :   9    0.00     10.00     -9999    33000 Hz coplanar quadra
         RES       :   9    0.00   1000.00     -9999    935 Hz resistivity (log(
         RES       :   9    0.00   1000.00     -9999    4600 Hz resistivity (log
         BLANK     :   9    0.00      0.00     -9999    Blank spacer record     
************************************************************************        
                                                                                
