 ********************************************************************************

                       Geosoft XYZ ARCHIVE SUMMARY                               
                       ---------------------------                               

 JOB TITLE:                                                                      
 ----------                                                                      

 JOB #              :1318
 TYPE OF SURVEY     :DIGHEM V EM, MAGNETICS, RESISTIVITY
 AREA               :BARB PROPERTY - FRANCES LAKE, YUKON
 CLIENT             :INTERNATIONAL BARYTEX RESOURCES LTD.

 ********************************************************************************

 FILE STRUCTURE:                                                                 
 ---------------                                                                 

 RECORDING                      :CD-ROM  
 SIZE/DENSITY                   :650 Mbyte                                        

 ********************************************************************************

 SURVEY DATA FORMAT:                                                             
 -------------------                                                             

   # PARAMETER TIME    UNITS         MULT   SUB  DEFAULT FORMAT       #   
   1 X         0.20   M              1.0     0        *  (F12.1)     12
   2 Y         0.20   M              1.0     0        *  (F12.1)     12
   3 FID       1.00                  1.0     0        *  (F8.1)       8
   4 BIRDHITE  0.20   FEET           1.0     0        *  (F8.1)       8
   5 MAG       0.20   NT             1.0     0        *  (F12.2)     12
   6 CXI900    0.20   PPM            1.0     0        *  (F8.1)       8
   7 CXQ900    0.20   PPM            1.0     0        *  (F8.1)       8
   8 CPI900    0.20   PPM            1.0     0        *  (F8.1)       8
   9 CPQ900    0.20   PPM            1.0     0        *  (F8.1)       8
  10 CXI5500   0.20   PPM            1.0     0        *  (F8.1)       8
  11 CXQ5500   0.20   PPM            1.0     0        *  (F8.1)       8
  12 CPI7200   0.20   PPM            1.0     0        *  (F8.1)       8
  13 CPQ7200   0.20   PPM            1.0     0        *  (F8.1)       8
  14 CPI56K    0.20   PPM            1.0     0        *  (F8.1)       8
  15 CPQ56K    0.20   PPM            1.0     0        *  (F8.1)       8
  16 RP900     0.20   OHM-M          1.0     0        *  (F10.1)     10
  17 RP7200    0.20   OHM-M          1.0     0        *  (F10.1)     10
  18 RP56K     0.20   OHM-M          1.0     0        *  (F10.1)     10
  19 DP900     0.20   M              1.0     0        *  (F10.1)     10
  20 DP7200    0.20   M              1.0     0        *  (F10.1)     10
  21 DP56K     0.20   M              1.0     0        *  (F10.1)     10
  22 DIFI      0.20   PPM            1.0     0        *  (F8.2)       8
  23 DIFQ      0.20   PPM            1.0     0        *  (F8.2)       8
  24 CDT       0.20   S              1.0     0        *  (F8.1)       8
  25 CPSP      0.20                  1.0     0        *  (F8.2)       8
  26 _4XSP     0.20                  1.0     0        *  (F8.2)       8
  27 _4XPL     0.20                  1.0     0        *  (F8.2)       8

 ********************************************************************************

 ISSUE DATE         :SEPTEMBER, 1998                                             
 FOR WHOM           :INTERNATIONAL BARYTEX RESOURCES LTD.                                            

 BY  WHOM           :GEOTERREX-DIGHEM a division of CGG Canada Ltd.             
                     2270 ARGENTIA ROAD, UNIT 2                                 
                     MISSISSAUGA, ONTARIO                                  
                     CANADA  L5N 6A6                                             
                     TEL. (905) 812-0212                                         
                     FAX  (905) 812-1504                                         
                                                                                 
                                                                                 
 PARAMETER DESCRIPTIONS :                                                        
   1 	X		UTM EASTING
   2 	Y		UTM NORTHING
   3 	FID		FIDUCIAL
   4 	BIRDHITE	BIRD TO EARTH SURFACE CLEARANCE
   5 	MAG		TOTAL MAGNETIC FIELD
   6 	CXI900		COAXIAL INPHASE     900 Hz
   7 	CXQ900		COAXIAL QUADRATURE  900 Hz
   8 	CPI900		COPLANAR INPHASE    900 Hz
   9 	CPQ900		COPLANAR QUADRATURE 900 Hz
  10 	CXI5500		COAXIAL INPHASE     5500 Hz
  11 	CXQ5500		COAXIAL QUADRATURE  5500 Hz
  12 	CPI7200		COPLANAR INPHASE    7200 Hz
  13 	CPQ7200		COPLANAR QUADRATURE 7200 Hz
  14 	CPI56K		COPLANAR INPHASE    56000 Hz
  15 	CPQ56K		COPLANAR QUADRATURE 56000 Hz
  16 	RP900		APPARENT RESISTIVITY 900 Hz
  17 	RP7200		APPARENT RESISTIVITY 7200 Hz
  18 	RP56K		APPARENT RESISTIVITY 56000 Hz
  19 	DP900		APPARENT DEPTH 900 Hz
  20 	DP7200		APPARENT DEPTH 7200 Hz
  21 	DP56K		APPARENT DEPTH 56000 Hz
  22 	DIFI		INPHASE DIFFERENCE 900 Hz COIL PAIR
  23 	DIFQ		QUADRATURE DIFFERENCE 900 Hz COIL PAIR
  24 	CDT		CONDUCTANCE GRADE
  25 	CPSP		COPLANAR ENVIRONMENTAL SPHERICS MONITOR
  26 	_4XSP		COAXIAL ENVIRONMENTAL SPHERICS MONITOR
  27 	_4XPL		COAXIAL POWER LINE MONITOR
