T1X - local grid coordinate of the stationary current electrode
T2X - local grid coordinate of the mobile current electrode
R1X - local grid coordinate of the first potential electrode
R2X - local grid coordinate of the second potential electrode
Vp - the primary voltage measured 1260 ms in the ontime window (mV)
I_mA - current (A)
Sp - Self potential (mV)
QC - quality control for IP
QC_RES - quality control for resistivity
IP[0] - Normalized Voltage measurement in the 40-80 ms offtime window (mV/V)
IP[1] - Normalized Voltage measurement in the 80-120 ms offtime window (mV/V)
IP[2] - Normalized Voltage measurement in the 120-160 ms offtime window (mV/V)
IP[3] - Normalized Voltage measurement in the 160-200 ms offtime window (mV/V)
IP[4] - Normalized Voltage measurement in the 200-240 ms offtime window (mV/V)
IP[5] - Normalized Voltage measurement in the 240-280 ms offtime window (mV/V)
IP[6] - Normalized Voltage measurement in the 280-360 ms offtime window (mV/V)
IP[7] - Normalized Voltage measurement in the 360-440 ms offtime window (mV/V)
IP[8] - Normalized Voltage measurement in the 440-520 ms offtime window (mV/V)
IP[9] - Normalized Voltage measurement in the 520-600 ms offtime window (mV/V)
IP[10] - Normalized Voltage measurement in the 600-680 ms offtime window (mV/V)
IP[11] - Normalized Voltage measurement in the 680-760 ms offtime window (mV/V)
IP[12] - Normalized Voltage measurement in the 760-840 ms offtime window (mV/V)
IP[13] - Normalized Voltage measurement in the 840-1000 ms offtime window (mV/V)
IP[14] - Normalized Voltage measurement in the 1000-1160 ms offtime window (mV/V)
IP[15] - Normalized Voltage measurement in the 1160-1320 ms offtime window (mV/V)
IP[16] - Normalized Voltage measurement in the 1320-1480 ms offtime window (mV/V)
IP[17] - Normalized Voltage measurement in the 1480-1640 ms offtime window (mV/V)
IP[18] - Normalized Voltage measurement in the 1640-1800 ms offtime window (mV/V)
IP[19] - Normalized Voltage measurement in the 1800-1960 ms offtime window (mV/V)
Q - error of the IP_Avg (mV/V)
Time - off-time length (ms)
Stack - number of cycles read
RsCheck - contact resistance of the potential electrodes (Ohm)
RxBat - Voltage of the receiver battery (V)
Date - date of data collection
DayTime - time of day of data collection
IP_Avg - the calculated area under the IP curve (mV/V)
N - Potential dipole separation from mobile current electrode / a
spacing
Stn - Local coordinate of the mid point between current and first
potential electrode.
X - Local coordinate of the Stn
Y - Line number
Z - Local Z coordinate of the plot point in pseudosection
Topo - Elevation of Stn (m)
Stn_UTME_NAD83_Z7 - Easting of Stn in NAD83, UTM Z7 coordinates
Stn_UTMN_NAD83_Z7 - Northing of Stn in NAD83, UTM Z7 coordinates
T1_UTME - NAD83 UTM Zone 7N Easting of T1X
T1_UTMN - NAD83 UTM Zone 7N Northing of T1X
T2_UTME - NAD83 UTM Zone 7N Easting of T2X
T2_UTMN - NAD83 UTM Zone 7N Northing of T2X
R1_UTME - NAD83 UTM Zone 7N Easting of R1X
R1_UTMN - NAD83 UTM Zone 7N Northing of R1X
R2_UTME - NAD83 UTM Zone 7N Easting of R2X
R2_UTMN - NAD83 UTM Zone 7N Northing of R2X
calcAppRes
T1_elevation - elevation of T1X proximal current electrode (metres above sea level)
T2_elevation - elevation of T1X proximal current electrode or infinite (metres above sea level)
R1_elevation - elevation of R1X (metres above sea level)
R2_elevation - elevation of R2X (metres above sea level)
IP_Er_Final - A weighted average of the standard deviation of each IP
measurement (mV/V)
Res_Final - A weighted average of the calculated apparent resistivity
(Ohm*m)
IP_Final - A weighted average of the IP measurement (mV/V)
