Archive Date: 2006-June-22
Archive Ref: CCD02446 
--------------------------------------------------------------------------------
This archive contains FINAL PROCESSED DATA
of an airborne geophysical survey flown by Fugro Airborne Surveys
on behalf of Cumberland Resources Ltd.
over the Tootsee River Property, British Columbia/Yukon Territory
in April, 2006

Job # 06030 

******* Disc 1 of 1 *******  

--------------------------------------------------------------------------------
This archive comprises 22 data files in the following four subdirectories:


Grids\ grids in Geosoft float format (*.grd) 

Tootsee_res400.grd  - apparent resistivity 400 Hz (ohm-m)
Tootsee_res1800.grd - apparent resistivity 1800 Hz (ohm-m)
Tootsee_res8200.grd - apparent resistivity 8200 Hz (ohm-m)
Tootsee_res40K.grd  - apparent resistivity 40K Hz (ohm-m)
Tootsee_res140K.grd - apparent resistivity 140K Hz (ohm-m)
Tootsee_tfmag.grd   - total magnetic field (nT)
Tootsee_cvg.grd     - calculated vertical gradient (nT/m)
Tootsee_dem.grd     - digital elevation model (m)


Linedata\ archive in Geosoft ASCII format


anTootsee.xyz - Geosoft ASCII .xyz anomaly data archive
Tootsee.xyz   - Geosoft ASCII .xyz data archive
Tootsee.txt   - archive text description file


PDF\ map products in Adobe Acrobat 4.0 format (*.pdf)

Tootsee_aema1_yukon.pdf     - Interpretated EM anomalies   - sheet 1
Tootsee_cvga1_yukon.pdf     - Calculated Vertical Gradient - sheet 1
Tootsee_maga1_yukon.pdf     - Total Magnetic Field         - sheet 1
Tootsee_res1800a1_yukon.pdf - Apparent Resistivity 1800 Hz - sheet 1
Tootsee_res8200a1_yukon.pdf - Apparent Resistivity 8200 Hz - sheet 1
Tootsee_aema2_bc.pdf        - Interpretated EM anomalies   - sheet 2
Tootsee_cvga2_bc.pdf        - Calculated Vertical Gradient - sheet 2
Tootsee_maga2_bc.pdf        - Total Magnetic Field         - sheet 2
Tootsee_res1800a2_bc.pdf    - Apparent Resistivity 1800 Hz - sheet 2
Tootsee_res8200a2_bc.pdf    - Apparent Resistivity 8200 Hz - sheet 2


REPORT\ report in Adobe Acrobat format

R06030Jun-22.pdf


--------------------------------------------------------------------------------
The coordinate system for all grids and archive files is projected as follows

Datum                               NAD83
Spheroid                            GRS80
Projection                          UTM Zone 9N
Central meridian                    -129 W
False easting                       500000
False northing                      0
Scale factor                        0.9996
Northern parallel                   N/A
Base parallel                       N/A
WGS84 to local conversion method    Molodensky
Delta X shift                       -0
Delta Y shift                       -0
Delta Z shift                       -0
--------------------------------------------------------------------------------
If you have any problems with this archive please contact

	Processing Manager
	FUGRO AIRBORNE SURVEYS CORP.
	2270 Argentia Road, Unit 2
	Mississauga, Ontario
	Canada    L5N 6A6
	Tel (905) 812-0212
	Fax (905) 812-1504
	E-mail toronto@fugroairborne.com