                      Geosoft XYZ ARCHIVE SUMMARY
                      -------------------------------
JOB TITLE:                                   
----------
JOB #              :06030
TYPE OF SURVEY     :FUGRO EM, MAGNETICS, RESISTIVITY
AREA               :Tootsee River Property, British Columbia/Yukon Territory
CLIENT             :Cumberland Resources Ltd.
****************************************************************************
SURVEY DATA FORMAT:
------------------- 
NUMBER OF DATA FIELDS :   36
  # CHANNAME(16LONG)  TIME   UNITS / DESCRIPTION            
  1 x                 0.1    m       easting   utme-nad83 (zone-9N)
  2 y                 0.1    m       northing  utmn-nad83 (zone-9N)
  3 fid               0.1            fiducial increment
  4 latitude          0.1    degrees latitude (NAD83)
  5 longitude         0.1    degrees longitude (NAD83)
  6 flight            0.1            flight number
  7 z                 0.1    m       GPS height above mean sea level
  8 altbird           0.1    m       radar height of bird above ground
  9 altlaser          0.1    m       laser height of bird above ground
 10 dem               0.1    m       digital elevation model
 11 diurnal_cor       0.1    nt      diurnal correction
 12 mag               0.1    nt      total magnetic field
 13 cpi400            0.1    ppm     coplanar inphase 386 Hz
 14 cpq400            0.1    ppm     coplanar quadrature 386 Hz
 15 cpi1800           0.1    ppm     coplanar inphase 1788 Hz
 16 cpq1800           0.1    ppm     coplanar quadrature 1788 Hz
 17 cxi3300           0.1    ppm     coaxial inphase 3245 Hz
 18 cxq3300           0.1    ppm     coaxial quadrature 3245 Hz
 19 cpi8200           0.1    ppm     coplanar inphase 8205 Hz
 20 cpq8200           0.1    ppm     coplanar quadrature 8205 Hz
 21 cpi40k            0.1    ppm     coplanar inphase 39850 Hz
 22 cpq40k            0.1    ppm     coplanar quadrature 39850 Hz
 23 cpi140k           0.1    ppm     coplanar inphase 132900 Hz
 24 cpq140k           0.1    ppm     coplanar quadrature 132900 Hz
 25 res400            0.1    ohm*m   resistivity coplanar 400 Hz
 26 res1800           0.1    ohm*m   resistivity coplanar 1800 Hz
 27 res8200           0.1    ohm*m   resistivity coplanar 8200 Hz
 28 res40k            0.1    ohm*m   resistivity coplanar 40k  Hz
 29 res140k           0.1    ohm*m   resistivity coplanar 140k Hz
 30 dep400            0.1    m       apparent depth of conductor 400 Hz
 31 dep1800           0.1    m       apparent depth of conductor 1800 Hz
 32 dep8200           0.1    m       apparent depth of conductor 8200 Hz
 33 dep40k            0.1    m       apparent depth of conductor 40k  Hz
 34 dep140k           0.1    m       apparent depth of conductor 140k Hz
 35 difi              0.1            diff. based on 3300/8200 inphase
 36 difq              0.1            diff. based on 3300/8200 quad   
****************************************************************************
ISSUE DATE         :June 22, 2006
FOR WHOM           :Cumberland Resources Ltd.
BY  WHOM           :FUGRO AIRBORNE SURVEYS
                    2270 ARGENTIA ROAD, UNIT 2
                    MISSISSAUGA, ONTARIO,
                    CANADA  L5N 6A6
                    TEL. (905) 812-0212
                    FAX (905) 812-1504