MAGNETOMETER DATA FILE – FORMAT (GEOSOFT GDB)

CHANNEL NAME  			DESCRIPTION 
RECS-Record Number
GTM_sec - GPS time
Xco_m - UTM Easting coordinate (WGS84/Zone8)
Yco_m - UTM Northing coordinate (WGS84/Zone8)
FinalMag - Final corrected Magnetometer value
Rad_feet - Radar Altitude in feet
Galt_m - Sensor Height in meters


SPECTROMETER DATA FILE – FORMAT (GEOSOFT GDB)

CHANNEL NAME  			DESCRIPTION
RECS - Record Number
GTM_sec - GPS time
Xco_m - UTM Easting coordinate (WGS84/Zone8)
Yco_m - UTM Northing coordinate (WGS84/Zone8)
Rad_feet - Radar Altitude in feet
Galt_m - Sensor Height in meter
TC_cps - Total count down
TCu_cps - Total count up
K_cps - Potassium window
UR_cps - Uranium down window
URu_cps - Uranium up window
Th_cps - Thorium window
Cos_cps - Cosmic window
Co_cps - Cobalt Window
Cs_cps - Cesium window
ISP1D_cps - Summed spectrum for downward looking crystal (256 resolution)
ISP1U_cps - Summed spectrum for upward looking crystal (256 resolution)
Baro_step - Barometric Pressure (mb)
HUMsp_proc - Humidity %
TMPsp_deg - Ambient Temperature (degrees C)

